
This directory contains line data extracted from the 2D-PIV
results:

x065off.dat  x066on.dat   x090off.dat   x100on.dat    x120off.dat   x130on.dat
x065on.dat   x080off.dat   x090on.dat    x110off.dat   x120on.dat
x066off.dat  x080on.dat    x100off.dat   x110on.dat    x130off.dat

where, for example, x065off.dat indicates data along a
vertical line at x/c=0.65, suction OFF, and x065on.dat
indicates data along a vertical line at x/c=0.65, suction ON.

This data includes both U/Uinf and V/Uinf, as well as
the turbulent stresses uu/Uinf^2, vv/Uinf^2, and uv/Uinf^2.
It was taken from 2D-PIV by extracting along an index 
of the PIV grid nearest to the desired x/c location.

It should be noted that the turbulence uv data has a maximum
error of as much as 20%, and urms and vrms have a maximum
error of as much as 14%, based on a pseudo-empirical
uncertainty analysis.  Therefore, the turbulence data given
here should not be taken as absolute levels, but rather
should be used to assist in qualitative evaluation of
turbulence models.

